Calibration

Different channels in the Tukan software corresponds to different energy levels of γ-radiation. But the relation is not linear so we need to calibrate so that every channel corresponds to the right energy level.

The calibration can be done in the software. First we